
|  |
| --- |
| **Recommended Installation Pump** |
| Our recommended pump is available for purchase for $550.00. For repeated use, Pump Flush must be used to completely clear the pump of all residue before and after each use. Klingstone Paths Pump Flush is available for $132.50 per 5 gallon pail. One application wand and uptake line are included with the aforementioned sale. Additional materials that installers will need are listed below. |

**Klingstone Paths Pump**

|  |  |
| --- | --- |
| **Additional Materials** | |
| Air Compressor | Minimum 18 gallon capacity, 8+ cfm rating |
| Air Compressor Hose | Standard ¼ inch connection |
| Standard Garden Hose | New, dry, 50 feet or less, 100 psi rating or higher, 5/8” thread |
| Uptake Lines | PVC construction, *included with pump purchase* |
| Application Wand | PVC construction, with ball valve attached, *included with pump purchase* |
| Safety Gear | See Safety Data Sheet (SDS) |

|  |
| --- |
| **Technical Information** |
| Non-metallic, air operated, double diaphragm pump |
| Capable output of 1–14.4 gallons per minute |
| Powered by an air compressor |
| 10-100 psi inlet/outlet pressure range |
| ¼ inch male connector to air compressor hose |
| Standard 5/8” “garden hose thread”, the hose connects the pump to the application wand |
| ½ inch PVC uptake lines |